{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Capacidad de refrigeración","Mín.","","kW","1.2"]
["","Máx.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Piping connections","Liquid","OD","mm","6.35"]
["","Gas","D.E.","mm","9.5"]
["","Drain","OD","mm","18.0"]
["Eficiencia nominal","Annual energy consumption","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","B"]
["","","Calefacción","","B"]
["Capacidad de calefacción","Nom.","","kW","4.0"]
["","Mín.","","kW","1.4"]
["","Máx.","","kW","5.0"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240V"]
["","","","","(5) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS, 24°CBH; longitud de tubería equivalente 5m"]
["","","","","(6) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m"]
["","","","","(7) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]