{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Nivel de presión sonora","Calefacción","Alto","dBA","46"]
["","","Funcionamiento silencioso","dBA","30"]
["","","Bajo","dBA","33"]
["","Refrigeración","Funcionamiento silencioso","dBA","29"]
["","","Bajo","dBA","32"]
["","","Alto","dBA","38"]
["","","Nom.","dBA","36"]
["","Refrigeración","Nom.","dBA","35"]
["Accesorios estándar","Manual de instalación","","","1"]
["","Manual de uso","","","1"]
["","Mando a distancia por infrarrojos","","","1"]
["","Pilas secas AAA","","","2"]
["","Soporte del mando a distancia","","","1"]
["","Placa de montaje","","","1"]
["","Tubo de aislamiento térmico (tubo de refrigerante)","","","8"]
["","Filtro purificador de aire","","","1"]
["","Filtro desodorizante fotocatalítico","","","1"]
["","Cubierta lateral","","","2"]
["","Banda de unión","","","4"]
["Sistemas de control","Infrared remote control","","","ARC433B67"]
["Conexiones de tubería","Liquid","OD","mm","6.35"]
["","Gas","D.E.","mm","9.5"]
["","Drain","","","18"]
["Sound power level","Refrigeración","","dBA","53"]
["","Calefacción","","dBA","59"]
["Dimensiones","Unidad","Anchura","mm","1,050"]
["","","Profundidad","mm","200"]
["","","Altura","mm","490"]
["Carcasa","Color","","","Blanco almendra"]
["Peso","Unidad","","kg","16"]
["Power supply","Fase","","","1~"]
["","Frecuencia","","Hz","50"]
["","Nombre","","","VM"]
["","Tensión","","V","220-240"]
["Notas","","","","(1) - 220 V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar."]