{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Nivel de presión sonora","Calefacción","Alto","dBA","42","44","46","39","40","41"]
["","","Funcionamiento silencioso","dBA","30","32","34","25","25","26"]
["","","Bajo","dBA","33","35","37","28","28","29"]
["","Refrigeración","Funcionamiento silencioso","dBA","31","33","34","22","22","23"]
["","","Bajo","dBA","34","36","37","25","26","27"]
["","","Alto","dBA","43","45","46","39","40","41"]
["","","Nom.","dBA","38","40","42","34","34","35"]
["","Refrigeración","Nom.","dBA","39","41","42","33","33","34"]
["Accesorios estándar","Manual de instalación","","","1","1","1","1","1","1"]
["","Manual de uso","","","1","1","1","1","1","1"]
["","Mando a distancia sin cable","","","1","1","1","1","1","1"]
["","Pilas","","","2","2","2","2","2","2"]
["","Soporte del mando a distancia","","","1","1","1","1","1","1"]
["","Placa de montaje","","","1","1","1","1","1","1"]
["","Tornillo de fijación de la unidad interior","","","","","","2","2","2"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","2","2","2","2","2","2"]
["Control systems","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Conexiones de tubería","Líquido","D.E.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","D.E.","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Drenaje","","","18","18","18","18","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Calefacción","Nom.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Nivel de potencia sonora","Refrigeración","","dBA","59","60","63","55","56","57"]
["","Calefacción","","dBA","58","59","62","55","56","57"]
["Dimensiones","Unidad","Anchura","mm","1,050","1,050","1,050","770","770","770"]
["","","Profundidad","mm","238","238","238","198","198","198"]
["","","Altura","mm","290","290","290","283","283","283"]
["Carcasa","Colour","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","12","12","12","7","7","7"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50","50","50","50"]
["","Nombre","","","V1","V1","V1","V1","V1","V1"]
["","Tensión","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Accesorios estándar","Tornillos de fijación de la unidad interior","","","2","2"]
["Notas","","","","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire.","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire.","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire."]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Accesorios estándar","Tornillos de fijación de la unidad interior (M4 x 12L)","","","","","2"]