{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Consumo","Refrigeración","","Nom.","kW","0.03","0.030","0.030"]
["","Calefacción","","Nom.","kW","0.04","0.040","0.040"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","198","198","198"]
["","","","Anchura","mm","770","770","770"]
["","","","Profundidad","mm","283","283","283"]
["Peso","Unidad","","","kg","7","7.00","7.00"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","9.1","9.2","9.3"]
["","","","Medio","m³/min","7.4","7.6","7.7"]
["","","","Bajo","m³/min","5.9","6.0","6.1"]
["","","","Funcionamiento silencioso","m³/min","4.7","4.8","4.9"]
["","","Calefacción","Alto","m³/min","9.4","9.7","10.1"]
["","","","Medio","m³/min","7.8","8.0","8.4"]
["","","","Bajo","m³/min","6.3","6.3","6.7"]
["","","","Funcionamiento silencioso","m³/min","5.5","5.5","5.7"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55","55","58"]
["","Calefacción","","","dBA","55","55","58"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","39","40","41"]
["","","","Medio","dBA","33","33","34"]
["","","","Bajo","dBA","25","26","27"]
["","","","Funcionamiento silencioso","dBA","22","22","23"]
["","Calefacción","","Alto","dBA","39","40","41"]
["","","","Medio","dBA","34","34","35"]
["","","","Bajo","dBA","28","28","29"]
["","","","Funcionamiento silencioso","dBA","25","25","26"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.50","9.50"]
["","Drenaje","","","","18","18","18"]
["Sistemas de control","Infrared remote control","","","","ARC433A87","ARC433A87","ARC433A87"]
["Accesorios estándar","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Alimentación eléctrica","Nombre","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240"]