{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":14,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-KV"]
[]
[]
[]
[]
["","","","","","FTX20K5V1B","FTX25K5V1B","FTX35K5V1B","FTX50K2V1B","FTX60K2V1B","FTX71K2V1B","FTX20K2V1B (Archived)","FTX25K2V1B (Archived)","FTX35K2V1B (Archived)"]
["Consumo","Refrigeración","","Nom.","kW","0.018","0.02","0.024","0.035","0.041","0.041","0.018","0.02","0.024"]
["","Calefacción","","Nom.","kW","0.022","0.023","0.029","0.038","0.044","0.044","0.022","0.023","0.029"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","286","286","286","295","295","295","286","286","286"]
["","","","Anchura","mm","770","770","770","990","990","990","770","770","770"]
["","","","Profundidad","mm","225","225","225","263","263","263","225","225","225"]
["Peso","Unidad","","","kg","8.5","8.5","9","13.5","13.5","13.5","8.5","8.5","9"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","9.9","10.4","11.8","16","17.6","17.6","9.9","10.4","11.8"]
["","","","Medio","m³/min","7.8","8","8.2","13.7","14.9","14.9","7.8","8","8.2"]
["","","","Bajo","m³/min","5.8","6.1","6.3","11.1","12.2","12.2","5.8","6.1","6.3"]
["","","","Funcionamiento silencioso","m³/min","4.8","4.8","4.9","10.1","11.2","11.2","4.8","4.8","4.9"]
["","","Calefacción","Alto","m³/min","10.9","11.1","12.8","16.7","18.9","18.9","10.9","11.1","12.8"]
["","","","Medio","m³/min","8.5","8.5","8.5","14.7","16.7","16.7","8.5","8.5","8.5"]
["","","","Bajo","m³/min","6.4","6.7","6.9","12.2","13.7","13.7","6.4","6.7","6.9"]
["","","","Funcionamiento silencioso","m³/min","5.2","5.2","5.2","10.9","12.1","12.1","5.2","5.2","5.2"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55","55","58","59","60","62","55","55","58"]
["","Calefacción","","","dBA","55","55","58","58","59","61","55","55","58"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","39","40","43","43","45","46","39","40","43"]
["","","","Medio","dBA","33","33","34","39","41","42","33","33","34"]
["","","","Bajo","dBA","25","26","27","34","36","37","25","26","27"]
["","","","Funcionamiento silencioso","dBA","20","20","20","31","33","34","20","20","20"]
["","Calefacción","","Alto","dBA","39","40","43","42","44","45","39","40","43"]
["","","","Medio","dBA","34","34","35","38","40","41","34","34","35"]
["","","","Bajo","dBA","28","28","29","33","35","36","28","28","29"]
["","","","Funcionamiento silencioso","dBA","23","23","26","30","32","33","23","23","26"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.5","9.5","12.7","12.7","12.7","9.5","9.5","9.5"]
["","Drenaje","","","","18","18","18","16","16","16","18","18","18"]
["Sistemas de control","Infrared remote control","","","","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11"]
["Sistemas de control","Controlador remoto con cable","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073","BRC944B2, BRC073","BRC944B2, BRC073","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accesorios estándar","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1"]
["Alimentación eléctrica","Nombre","","","","V1","V1","V1","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]