{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","39","40"]
["","","Medio","dBA","34","34"]
["","","Funcionamiento silencioso","dBA","21","21"]
["","","Bajo","dBA","28","28"]
["","Refrigeración","Medio","dBA","33","33"]
["","","Funcionamiento silencioso","dBA","20","20"]
["","","Bajo","dBA","25","26"]
["","","Alto","dBA","39","40"]
["Accesorios estándar","Manual de instalación","","","1","1"]
["","Manual de uso","","","1","1"]
["","Mando a distancia por infrarrojos","","","1","1"]
["","Pilas secas AAA","","","2","2"]
["","Soporte del mando a distancia","","","1","1"]
["","Placa de montaje","","","1","1"]
["","Tornillos de fijación de la unidad interior","","","2","2"]
["Sistemas de control","Controlador remoto con cable","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Conexiones de tubería","Líquido","D.E.","mm","6.35","6.35"]
["","Gas","D.E.","mm","9.50","9.50"]
["","Drenaje","","","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.017","0.019"]
["","Calefacción","Nom.","kW","0.020","0.020"]
["Nivel de potencia sonora","Refrigeración","","dBA","55","55"]
["","Calefacción","","dBA","55","55"]
["Dimensiones","Unidad","Anchura","mm","770","770"]
["","","Profundidad","mm","225","225"]
["","","Altura","mm","286","286"]
["Carcasa","Color","","","Blanco","Blanco"]
["Peso","Unidad","","kg","8.50","8.50"]
["Power supply","Fase","","","1~","1~"]
["","Frecuencia","","Hz","50","50"]
["","Tensión","","V","220-240","220-240"]