{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F / 2MXF-B"]
[]
[]
[]
[]
["","","","","FTXF20F5V1B / FTXF20F5V1B / 2MXF40B2V1B","FTXF25F5V1B / FTXF25F5V1B / 2MXF50B2V1B"]
["Capacidad de refrigeración","Mín.","","kW","1.50","1.80"]
["","Nom.","","kW","4.00","5.00"]
["","Máx.","","kW","4.20","5.40"]
["Capacidad de calefacción","Mín.","","kW","1.30","1.20"]
["","Nom.","","kW","4.20","5.60"]
["","Máx.","","kW","4.60","6.00"]
["Eficiencia nominal","EER","","","3.90","3.37"]
["","COP","","","4.10","3.71"]
["","Consumo energético anual","","kWh","513","742"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A"]
["","","Calefacción","","A","A"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A++","A++"]
["","Capacidad","Pdesign","kW","4.00","5.00"]
["","SEER","","","7.50","7.85"]
["","Consumo energético anual","","kWh/a","187","223"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A++","A++"]
["","Capacidad","Pdesign","kW","3.20","4.20"]
["","SCOP/A","","","4.62","4.61"]
["","Capacidad de calefacción Pdh a -10°","","kW","2.79","3.32"]
["","Consumo energético anual","","kWh/a","970","1275"]