{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BB / RXJ20M5V1B9","FTXJ25A2V1BB / RXJ25M5V1B9","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ35A2V1BB / RXJ35M5V1B9"]
["Capacidad de refrigeración","Nom.","","kW","","","3.50"]
["Eficiencia nominal","Annual energy consumption","","kWh","","","428"]
["","EER","","","","","4.09"]
["","COP","","","","","4.04"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","A"]
["","","Calefacción","","","","A"]
["Capacidad de calefacción","Nom.","","kW","","","4.00"]
["Notas","","","","","","(1) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","","(2) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","","","(3) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","","","(4) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["Outdoor unit","","","","RXJ20M5V1B9","RXJ25M5V1B9","","RXJ35M5V1B9"]
["Capacidad de refrigeración","Nom.","","kW","2.30","2.40","","3.50"]
["Capacidad de calefacción","Nom.","","kW","2.50","3.20","","4.00"]
["Eficiencia nominal","EER","","","4.64","4.73","","4.09"]
["","COP","","","5.00","4.57","","4.04"]
["","Consumo energético anual","","kWh","248","254","","428"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","","A"]
["","","Calefacción","","A","A","","A"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A+++","A+++","","A++"]
["","Capacidad","Pdesign","kW","2.30","2.40","","3.50"]
["","SEER","","","8.73","8.64","","7.19"]
["","Consumo energético anual","","kWh/a","92","97","","170"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A++","A++","","A++"]
["","Capacidad","Pdesign","kW","2.10","2.70","","3.00"]
["","SCOP/A","","","4.61","4.60","","4.60"]
["","Capacidad de calefacción Pdh a -10°","","kW","1.80","2.18","","2.61"]
["","Consumo energético anual","","kWh/a","638","822","","913"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]