{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Capacidad de refrigeración","Nom.","","kW","4.00","4.00","4.00","5.20","4.00","6.00"]
["Eficiencia nominal","Consumo energético anual","","kWh","467","482","471","593","457","787"]
["","EER","","","4.28","4.15","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","3.95","4.05","4.42","4.04","3.88"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","A","A","A","A"]
["","","Calefacción","","A","A","A","A","A","A"]
["Capacidad de calefacción","Nom.","","kW","4.60","4.60","6.80","6.80","6.50","7.80"]
["Notas","","","","","(1) - Capacidades nom. de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(4) - Consulte en el plano independiente con los datos eléctricos."]