{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":14,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / RXJ20M2V1B","FTXJ20MV1BW / RXJ20M3V1B","FTXJ20MV1BW / RXJ20M5V1B","FTXJ25MV1BW / RXJ25M2V1B","FTXJ25MV1BW / RXJ25M3V1B","FTXJ25MV1BW / RXJ25M5V1B","FTXJ35MV1BW / RXJ35M5V1B","FTXJ35MV1BW / RXJ35M2V1B","FTXJ35MV1BW / RXJ35M3V1B","FTXJ50MV1BW / RXJ50MV1B"]
["Capacidad de refrigeración","Mín.","","kW","","1.30","","","0.90","","","","0.90"]
["","Máx.","","kW","","2.80","","","3.30","","","","4.10"]
["","Nom.","","kW","2.3","2.30","2.30","2.4","2.40","2.40","3.50","3.5","3.50","4.80"]
["Eficiencia nominal","Annual energy consumption","","kWh","248","248","248","254","254","254","428","428","428","716"]
["","EER","","","4.64","4.64","4.64","4.73","4.73","4.73","4.09","4.09","4.09","3.35"]
["","COP","","","5.00","5.00","5.00","4.57","4.57","4.57","4.04","4.04","4.04","3.65"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","A","A","A","A","A","A","A","A"]
["","","Calefacción","","A","A","A","A","A","A","A","A","A","A"]
["Capacidad de calefacción","Nom.","","kW","2.5","2.50","2.5","3.2","3.20","3.2","4.0","4","4.00","5.80"]
["","Mín.","","kW","","1.30","","","0.90","","","","0.90"]
["","Máx.","","kW","","4.30","","","4.70","","","","5.10"]
["Notas","","","","","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]
["","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]