{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Unidad exterior","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Capacidad de refrigeración","Mín.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Máx.","","kW","","3.0"]
["Capacidad de calefacción","Mín.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Máx.","","kW","","4.00"]
["Eficiencia nominal","Consumo energético anual","","kWh","","326"]
["","COP","","","","4.36"]
["","EER","","","","3.83"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","A"]
["","","Calefacción","","","A"]
["Notas","","","","","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","","(3) - Consulte en el plano independiente con los datos eléctricos."]
["Capacidad de refrigeración","Mín.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Máx.","","kW","2.6","","4.0"]
["Capacidad de calefacción","Mín.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Máx.","","kW","3.50","","4.80"]
["Eficiencia nominal","EER","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Consumo energético anual","","kWh","249"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","","A"]
["","","Calefacción","","A","","A"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A++","","A++"]
["","Capacidad","Pdesign","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Consumo energético anual","","kWh/a","103","","186"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A++","","A++"]
["","Capacidad","Pdesign","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Capacidad de calefacción Pdh a -10°","","kW","1.99","","2.33"]
["","Consumo energético anual","","kWh/a","662","","845"]
["Rango de eficiencia energética","","","","A+++ ~ D","","A+++ ~ D"]