{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":7,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXQ-A"]
[]
[]
[]
[]
["","","","","","FTXQ25AMV1B","FTXQ35AMV1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","42.0"]
["","","","Medio","dBA","","35.0"]
["","","","Funcionamiento silencioso","dBA","","25.0"]
["","","","Bajo","dBA","","30.0"]
["","Refrigeración","","Medio","dBA","","35.0"]
["","","","Funcionamiento silencioso","dBA","","24.0"]
["","","","Bajo","dBA","","28.0"]
["","","","Alto","dBA","","41.0"]
["Accesorios estándar","Manual de instalación","","","","","1"]
["","Manual de uso","","","","","1"]
["","Pilas secas AAA","","","","","2"]
["","Placa de montaje","","","","","1"]
["","Tornillos de fijación de la unidad interior","","","","","2"]
["","Precauciones generales de seguridad","","","","","1"]
["","Mando a distancia por infrarrojos","","","","","1"]
["","Soporte del mando a distancia","","","","","1"]
["Sistemas de control","Infrared remote control","","","","","ARC470A1"]
["Conexiones de tubería","Liquid","","OD","mm","","6.35"]
["","Gas","","D.E.","mm","","9.50"]
["","Drain","","","","","18"]
["Consumo","Refrigeración","","Nom.","kW","","0.025"]
["","Calefacción","","Nom.","kW","","0.031"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","55"]
["Dimensiones","Unidad","","Anchura","mm","","770"]
["","","","Profundidad","mm","","232"]
["","","","Altura","mm","","291"]
["Carcasa","Color","","","","","Blanco"]
["Peso","Unidad","","","kg","","9.00"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","12.0"]
["","","","Bajo","m³/min","","8.3"]
["","","","Medio","m³/min","","10.0"]
["","","","Funcionamiento silencioso","m³/min","","6.9"]
["","","Refrigeración","Bajo","m³/min","","7.0"]
["","","","Medio","m³/min","","8.5"]
["","","","Alto","m³/min","","10.5"]
["","","","Funcionamiento silencioso","m³/min","","6.0"]
["Power supply","Fase","","","","","1~"]
["","Frecuencia","","","Hz","","50"]
["","Tensión","","","V","","220-240"]
["Notas","","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS, 24°CBH; longitud de tubería equivalente 5m"]
["","","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m"]
["Consumo","Refrigeración","","Nom.","kW","0.023"]
["","Calefacción","","Nom.","kW","0.027"]
["Carcasa","Color","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","291"]
["","","","Anchura","mm","770"]
["","","","Profundidad","mm","232"]
["Peso","Unidad","","","kg","9"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","10.2"]
["","","","Medio","m³/min","8.1"]
["","","","Bajo","m³/min","6.5"]
["","","","Funcionamiento silencioso","m³/min","5"]
["","","Calefacción","Alto","m³/min","11.1"]
["","","","Medio","m³/min","9.6"]
["","","","Bajo","m³/min","8.1"]
["","","","Funcionamiento silencioso","m³/min","6.8"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","40"]
["","","","Medio","dBA","34"]
["","","","Bajo","dBA","26"]
["","","","Funcionamiento silencioso","dBA","23"]
["","Calefacción","","Alto","dBA","40"]
["","","","Medio","dBA","34"]
["","","","Bajo","dBA","29"]
["","","","Funcionamiento silencioso","dBA","25"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35"]
["","Gas","","D.E.","mm","9.5"]
["","Drenaje","","","","18"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","ARC470A1"]
["Accesorios estándar","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]