{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F8"]
[]
[]
[]
[]
["","","","","FTXS71GV1B / RXS71FAV1B8"]
["Capacidad de refrigeración","Mín.","","kW","2.3"]
["","Máx.","","kW","8.5"]
["","Nom.","","kW","7.10"]
["Conexiones de tubería","Líquido","D.E.","mm","6.35"]
["","Gas","D.E.","mm","15.9"]
["","Drenaje","D.E.","mm","18"]
["Eficiencia nominal","Consumo energético anual","","kWh","1,175"]
["","EER","","","3.02"]
["","COP","","","3.22"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","B"]
["","","Calefacción","","C"]
["Capacidad de calefacción","Nom.","","kW","8.20"]
["","Mín.","","kW","2.3"]
["","Máx.","","kW","10.2"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240V"]
["","","","","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]