{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","38","39","42","42","44","","46"]
["","","","Funcionamiento silencioso","dBA","25","25","26","30","31","","34"]
["","","","Bajo","dBA","28","28","29","33","34","","37"]
["","Refrigeración","","Funcionamiento silencioso","dBA","22","22","23","30","31","","34"]
["","","","Bajo","dBA","25","25","26","33","34","","37"]
["","","","Alto","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Refrigeración","","Nom.","dBA","32","32","34","38","39","","42"]
["Accesorios estándar","Filtro purificador de aire fotocatalítico de apatito de titanio","","","","2","2","2","2","2"]
["","Manual de uso","","","","1","1","1","1","1","","1"]
["","Manual de instalación","","","","1","1","1","1","1","","1"]
["","Mando a distancia sin cable","","","","1","1","1","1","1","","1"]
["","Pilas","","","","2","2","2","2","2","","2"]
["","Soporte del mando a distancia","","","","1","1","1","1","1","","1"]
["","Tornillos de fijación de la unidad interior","","","","2","2","2","2","2","","2"]
["","Placa de montaje","","","","1","1","1","1","1","","1"]
["Sistemas de control","Infrared remote control","","","","","","","","","","ARC452A3"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gas","","D.E.","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Drain","","","","18","18","18","18","18","","18"]
["Consumo","Refrigeración","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Calefacción","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","54","54","58","58","59","","63"]
["","Calefacción","","","dBA","54","55","58","58","60","","62"]
["Dimensiones","Unidad","","Anchura","mm","800","800","800","800","800","","1,050"]
["","","","Profundidad","mm","215","215","215","215","215","","250"]
["","","","Altura","mm","295","295","295","295","295","","290"]
["Carcasa","Colour","","","","Blanco","Blanco","Blanco","Blanco","Blanco","","Blanco"]
["Peso","Unidad","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","","50"]
["","Nombre","","","","V1","V1","V1","V1","V1","","V1"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Notas","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire."]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Ventilador","Caudal de aire","Refrigeración","Nom.","m³/min","","","","","","16.0"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","","","","","","41"]
["Ventilador","Caudal de aire","Calefacción","Nom.","m³/min","","","","","","14.9"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","","","","","","40"]
["Consumo","Refrigeración","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Calefacción","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Carcasa","Color","","","","","","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","","","","","","290"]
["","","","Anchura","mm","","","","","","1050"]
["","","","Profundidad","mm","","","","","","250"]
["Peso","Unidad","","","kg","","","","","","12"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","","","","","16.0"]
["","","","Bajo","m³/min","","","","","","11.3"]
["","","","Funcionamiento silencioso","m³/min","","","","","","10.1"]
["","","Calefacción","Alto","m³/min","","","","","","17.2"]
["","","","Bajo","m³/min","","","","","","12.6"]
["","","","Funcionamiento silencioso","m³/min","","","","","","11.3"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","","","","60"]
["","Calefacción","","","dBA","","","","","","59"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","","","","","45"]
["","","","Bajo","dBA","","","","","","36"]
["","","","Funcionamiento silencioso","dBA","","","","","","33"]
["","Calefacción","","Alto","dBA","","","","","","44"]
["","","","Bajo","dBA","","","","","","35"]
["","","","Funcionamiento silencioso","dBA","","","","","","32"]
["Conexiones de tubería","Líquido","","D.E.","mm","","","","","","6.35"]
["","Gas","","D.E.","mm","","","","","","12.7"]
["","Drenaje","","","","","","","","","18"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","","","","","","ARC452A3"]
["Accesorios estándar","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Alimentación eléctrica","Nombre","","","","","","","","","V1"]
["","Fase","","","","","","","","","1~"]
["","Frecuencia","","","Hz","","","","","","50"]
["","Tensión","","","V","","","","","","220-240"]
["Accesorios estándar","Filtro purificador de aire fotocatalítico de apatito de titanio sin marco","","","","","","","","","","2"]
["Notas","","","","","","","","","","","(4) - 240V"]