{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L2V1B","FTXS25K2V1B / RXS25L2V1B","FTXS35K2V1B / RXS35L2V1B","FTXS42K2V1B / RXS42L2V1B","FTXS42K3V1B / RXS42L2V1B","FTXS50K2V1B / RXS50L2V1B","FTXS50K3V1B / RXS50L2V1B"]
["Capacidad de refrigeración","Mín.","","kW","1.3","1.3","1.4","1.7","","1.7"]
["","Máx.","","kW","2.8","3.2","4.0","5.0","","5.3"]
["","Nom.","","kW","2.00","2.5","3.5","4.20","","5.00"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35","6.35","","6.35"]
["","Gas","D.E.","mm","9.5","9.5","9.5","9.5","","12.7"]
["","Drain","OD","mm","18","18","18","18","","18"]
["Eficiencia nominal","Annual energy consumption","","kWh","215","285","430","590","","705"]
["","EER","","","4.65","4.39","4.07","3.56","","3.55"]
["","COP","","","4.72","4.67","4.76","4.12","","4.00"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","A","A","","A"]
["","","Calefacción","","A","A","A","A","","A"]
["Capacidad de calefacción","Nom.","","kW","2.5","2.8","4.00","5.40","","5.80"]
["","Mín.","","kW","1.3","1.3","1.4","1.7","","1.7"]
["","Máx.","","kW","4.3","4.7","5.2","6.0","","6.5"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - 220 V","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 220 V","(3) - 230V","(3) - 220 V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 230V","(4) - 240V","(4) - 230V"]
["","","","","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(5) - 240V","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(5) - 240V"]
["Outdoor unit","","","","","","","","RXS42L","","RXS50L"]
["Capacidad de refrigeración","Mín.","","kW","","","","","1.7","","1.7"]
["","Nom.","","kW","","","","","4.20","","5.00"]
["","Máx.","","kW","","","","","5.0","","5.3"]
["Capacidad de calefacción","Mín.","","kW","","","","","1.7","","1.7"]
["","Nom.","","kW","","","","","5.40","","5.80"]
["","Máx.","","kW","","","","","6.0","","6.5"]
["Eficiencia nominal","EER","","","","","","","3.35","","3.32"]
["","COP","","","","","","","4.12","","4.00"]
["","Consumo energético anual","","kWh","","","","","627","","753"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","","","A","","A"]
["","","Calefacción","","","","","","A","","A"]
["Conexiones de tubería","Drenaje","D.E.","mm","","","","","18","","18"]
["","Gas","D.E.","mm","","","","","12.7","","12.7"]
["","Líquido","D.E.","mm","","","","","6.35","","6.35"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","","","","","A++","","A++"]
["","Capacidad","Pdesign","kW","","","","","4.20","","5.00"]
["","SEER","","","","","","","6.80","","6.80"]
["","Consumo energético anual","","kWh/a","","","","","216","","257"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","","","","","A+","","A+"]
["","Capacidad","Pdesign","kW","","","","","4.00","","4.60"]
["","SCOP/A","","","","","","","4.20","","4.20"]
["","Consumo energético anual","","kWh/a","","","","","1334","","1535"]