{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L3"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L3V1B","FTXS20K3V1B / RXS20L3V1B","FTXS25K2V1B / RXS25L3V1B","FTXS25K3V1B / RXS25L3V1B","FTXS35K2V1B / RXS35L3V1B","FTXS35K3V1B / RXS35L3V1B"]
["Capacidad de refrigeración","Mín.","","kW","","","","","","1.4"]
["","Máx.","","kW","","","","","","4.0"]
["","Nom.","","kW","2.0","2.00 (2)","2.5","2.5 (2)","3.5","3.5 (2)"]
["Conexiones de tubería","Líquido","D.E.","mm","","6.35","","6.35","","6.35"]
["","Gas","D.E.","mm","","9.5","","9.5","","9.5"]
["","Drenaje","OD","mm","","18","","18","","18"]
["Eficiencia nominal","Consumo energético anual","","kWh","228","228","297","297","450","450"]
["","EER","","","4.39","4.39 (1)","4.21","4.21 (1)","3.89","3.89 (1)"]
["","COP","","","4.72","4.72 (1)","4.67","4.67 (1)","4.76","4.76 (1)"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","A","A","A","A"]
["","","Calefacción","","A","A","A","A","A","A"]
["Capacidad de calefacción","Nom.","","kW","2.5","2.5 (2)","2.8","2.8 (2)","4.0","4.00 (2)"]
["","Mín.","","kW","","1.3","","1.3","","1.4"]
["","Máx.","","kW","","4.3","","4.7","","5.2"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]
["","","","","","(3) - 220 V","","(3) - 220 V","","(3) - 220 V"]
["","","","","","(4) - 230V","","(4) - 230V","","(4) - 230V"]
["","","","","","(5) - 240V","","(5) - 240V","","(5) - 240V"]