{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","40","","","","","","45"]
["","","","Funcionamiento silencioso","dBA","19","","","","","","22"]
["","","","Bajo","dBA","27","","","","","","33"]
["","Refrigeración","","Funcionamiento silencioso","dBA","19","","","","","","21"]
["","","","Bajo","dBA","24","","","","","","33"]
["","","","Alto","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Refrigeración","","Nom.","dBA","32","","","","","","39"]
["Accesorios estándar","Manual de instalación","","","","1","","","","","","1"]
["","Manual de uso","","","","1","","","","","","1"]
["","Mando a distancia sin cable","","","","1","","","","","","1"]
["","Pilas","","","","2","","","","","","2"]
["","Soporte del mando a distancia","","","","1","","","","","","1"]
["","Placa de montaje","","","","1","","","","","","1"]
["","Tornillos de fijación de la unidad interior","","","","2","","","","","","2"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","","2","","","","","","2"]
["Sistemas de control","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","","","","","","6.35"]
["","Gas","","D.E.","mm","9.5","","","","","","9.5"]
["","Drain","","","","18","","","","","","18"]
["Consumo","Refrigeración","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Calefacción","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","58","","","","","","59"]
["","Calefacción","","","dBA","58","","","","","","59"]
["Dimensiones","Unidad","","Anchura","mm","780","","","","","","900"]
["","","","Profundidad","mm","215","","","","","","215"]
["","","","Altura","mm","289","","","","","","298"]
["Carcasa","Colour","","","","Blanco","","","","","","Blanco"]
["Peso","Unidad","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Frecuencia","","","Hz","50","","","","","","50"]
["","Nombre","","","","V1","","","","","","V1"]
["","Tensión","","","V","220-240","","","","","","220-240"]
["Notas","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220 V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Consumo","Refrigeración","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Calefacción","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Carcasa","Color","","","","","Blanco","Blanco","Blanco","Blanco","Blanco","","Blanco","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","","215","289","215","298","215","","215","298","215"]
["","","","Anchura","mm","","780","780","780","900","900","","900","900","900"]
["","","","Profundidad","mm","","289","215","289","215","298","","298","215","298"]
["Peso","Unidad","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Medio","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Bajo","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Funcionamiento silencioso","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Calefacción","Alto","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Medio","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Bajo","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Funcionamiento silencioso","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Calefacción","","","dBA","","58","58","58","59","59","","59","60","60"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Medio","dBA","","32","33","33","","37","","39","","40"]
["","","","Bajo","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Funcionamiento silencioso","dBA","","19","19","19","19","19","","21","23","23"]
["","Calefacción","","Alto","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Medio","dBA","","34","34","34","","39","","39","","40"]
["","","","Bajo","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Funcionamiento silencioso","dBA","","19","19","19","19","19","","22","24","24"]
["Conexiones de tubería","Líquido","","D.E.","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Drenaje","","","","","18","18","18","18","18","","18","18","18"]
["Sistemas de control","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Accesorios estándar","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Alimentación eléctrica","Nombre","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frecuencia","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Tensión","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilador","Caudal de aire","Refrigeración","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilador","Caudal de aire","Calefacción","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","","","34","","39","","","","40"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Accesorios estándar","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Notas","","","","","","","","","","","(4) - 240V"]