{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Consumo","Refrigeración","","Nom.","kW","0.035","0.053"]
["","Calefacción","","Nom.","kW","0.039","0.06"]
["Carcasa","Color","","","","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","295","299"]
["","","","Anchura","mm","778","998"]
["","","","Profundidad","mm","272","292"]
["Peso","Unidad","","","kg","10","15"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","11.5","15.1"]
["","","","Medio","m³/min","7.5","9.2"]
["","","","Bajo","m³/min","5.2","5.6"]
["","","","Funcionamiento silencioso","m³/min","4.2","4.8"]
["","","Calefacción","Alto","m³/min","11.6","17"]
["","","","Medio","m³/min","7.3","10"]
["","","","Bajo","m³/min","4.7","6"]
["","","","Funcionamiento silencioso","m³/min","4","5.1"]
["Nivel de potencia sonora","Refrigeración","","","dBA","60","60"]
["","Calefacción","","","dBA","60","60"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","45","46"]
["","","","Medio","dBA","33","32"]
["","","","Bajo","dBA","25","24"]
["","","","Funcionamiento silencioso","dBA","21","20"]
["","Calefacción","","Alto","dBA","45","46"]
["","","","Medio","dBA","31","31"]
["","","","Bajo","dBA","22","22"]
["","","","Funcionamiento silencioso","dBA","19","19"]
["Refrigerante","GWP","","","","675","675"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.5"]
["","Drenaje","","","","18","18"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","ARC466A83","ARC466A83"]
["","Controlador remoto con cable","","","","BRC073A1","BRC073A1"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]