{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":10,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N / RXZ-N"]
[]
[]
[]
[]
["","","","","FTXZ25NV1B / RXZ25NV1B","FTXZ25NV1B / RXZ25NV1B9","FTXZ35NV1B / RXZ35NV1B","FTXZ35NV1B / RXZ35NV1B9","FTXZ50NV1B / RXZ50NV1B9","FTXZ50NV1B / RXZ50NV1B"]
["Capacidad de refrigeración","Mín.","","kW","0.6","0.6","0.6","0.6","0.6"]
["","Máx.","","kW","3.9","3.9","5.3","5.3","5.8"]
["","Nom.","","kW","2.5","2.5","3.5","3.5","5.0"]
["Conexiones de tubería","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","D.E.","mm","9.5","9.5","9.5","9.5","9.5"]
["Eficiencia nominal","Annual energy consumption","","kWh","205","205","330","330","550"]
["","EER","","","6.10","6.10","5.30","5.30","4.55"]
["","COP","","","5.80","5.80","5.00","5.00","4.47"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","A","A","A"]
["","","Calefacción","","A","A","A","A","A"]
["Capacidad de calefacción","Nom.","","kW","3.6","3.6","5.0","5.0","6.3"]
["","Mín.","","kW","0.6","0.6","0.6","0.6","0.6"]
["","Máx.","","kW","7.5","7.5","9.0","9.0","9.4"]
["Notas","","","","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(1) - 230V"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 240V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]
["Capacidad de refrigeración","Mín.","","kW","","","","","","0.6"]
["","Nom.","","kW","","","","","","5.0"]
["","Máx.","","kW","","","","","","5.8"]
["Capacidad de calefacción","Mín.","","kW","","","","","","0.6"]
["","Nom.","","kW","","","","","","6.3"]
["","Máx.","","kW","","","","","","9.4"]
["Eficiencia nominal","EER","","","","","","","","4.55"]
["","COP","","","","","","","","4.47"]
["","Consumo energético anual","","kWh","","","","","","550"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","","","","A"]
["","","Calefacción","","","","","","","A"]
["Conexiones de tubería","Gas","D.E.","mm","","","","","","9.5"]
["","Líquido","D.E.","mm","","","","","","6.35"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","","","","","","A+++"]
["","Capacidad","Pdesign","kW","","","","","","5.00"]
["","SEER","","","","","","","","8.60"]
["","Consumo energético anual","","kWh/a","","","","","","203"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","","","","","","A+++"]
["","Capacidad","Pdesign","kW","","","","","","5.60"]
["","SCOP/A","","","","","","","","5.50"]
["","Consumo energético anual","","kWh/a","","","","","","1427"]