{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","","","41","46","47"]
["","","","Medio","dBA","","","","38","42","43"]
["","","","Bajo","dBA","","","","35","39","40"]
["","Refrigeración","","Medio","dBA","","","","38","42","43"]
["","","","Bajo","dBA","","","","35","39","40"]
["","","","Alto","dBA","","","","41","46","47"]
["Accesorios estándar","Manual de uso","","","","","","","1","1","1"]
["","Manual de instalación","","","","","","","1","1","1"]
["","Tubo flexible de drenaje","","","","","","","1","1","1"]
["","Tubo de aislamiento térmico","","","","","","","3","3","3"]
["","Arrollamientos de unión","","","","","","","10","10","10"]
["","Abrazadera de tubo flexible","","","","","","","1","1","1"]
["","Material de sellado","","","","","","","4","4","4"]
["","Arandela para placa de fijación","","","","","","","1","1","1"]
["","Junta de drenaje","","","","","","","1","1","1"]
["","Tela no tejida","","","","","","","1","1","1"]
["","Arandela","","","","","","","8","8","8"]
["","Tornillo de fijación del tubo de drenaje","","","","","","","5","5","5"]
["Sistemas de control","Controlador remoto con cable","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","","","","","","12.1"]
["Conexiones de tubería","Liquid","","OD","mm","","","","9.52","9.52","9.52"]
["","Gas","","D.E.","mm","","","","15.9","15.9","15.9"]
["","Drain","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","","59","64","65"]
["","Calefacción","","","dBA","","","","59","64"]
["Dimensiones","Unidad","","Anchura","mm","","","","950","950","950"]
["","","","Profundidad","mm","","","","950","950","950"]
["","","","Altura","mm","","","","198","198","198"]
["Carcasa","Material","","","","","","","Resina","Resina","Resina"]
["","Color","","","","","","","Blanco fresco","Blanco fresco","Blanco fresco"]
["Peso","Unidad","","","kg","","","","25.0","26.0","26"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","","","23.0","31.0","32.5"]
["","","","Medio","m³/min","","","","19.5","25.5","26.5"]
["","","","Bajo","m³/min","","","","16.0","20.0","20.5"]
["","","Refrigeración","Bajo","m³/min","","","","16.0","20.0","20.5"]
["","","","Medio","m³/min","","","","19.5","25.5","26.5"]
["","","","Alto","m³/min","","","","23.0","31.0","32.5"]
["Altura de drenaje","mm","","","","","","","600","600","600"]
["Capacidad de calefacción","Capacidad total","","Nom.","kW","","","","","","13.5"]
["Carcasa","Color","","","","Blanco fresco","Blanco fresco","Blanco fresco"]
["","Material","","","","Resina","Resina","Resina"]
["Dimensiones","Unidad","","Altura","mm","198","198","198"]
["","","","Anchura","mm","950","950","950"]
["","","","Profundidad","mm","950","950","950"]
["Peso","Unidad","","","kg","25.0","26.0","26.0"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","23.0","31.0","32.5"]
["","","","Medio","m³/min","19.5","25.5","26.5"]
["","","","Bajo","m³/min","16.0","20.0","20.5"]
["","","Calefacción","Alto","m³/min","23.0","31.0","32.5"]
["","","","Medio","m³/min","19.5","25.5","26.5"]
["","","","Bajo","m³/min","16.0","20.0","20.5"]
["Nivel de potencia sonora","Refrigeración","","","dBA","59","64","65"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","41","46","47"]
["","","","Medio","dBA","38","42","43"]
["","","","Bajo","dBA","35","39","40"]
["","Calefacción","","Alto","dBA","41","46","47"]
["","","","Medio","dBA","38","42","43"]
["","","","Bajo","dBA","35","39","40"]
["Conexiones de tubería","Líquido","","D.E.","mm","9.52","9.52","9.52"]
["","Gas","","D.E.","mm","15.9","15.9","15.9"]
["","Drenaje","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Altura de drenaje","mm","","","","600","600","600"]
["Accesorios estándar","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","","","12.10"]
["Capacidad de calefacción","Capacidad total","","Nom.","kW","","","13.5"]