{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":69,"n_cols":8,"rows_kept":69,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXM-ATV3"]
[]
[]
[]
[]
["","","","","","FWXM10AATV3","FWXM15AATV3","FWXM20AATV3"]
["Capacidad de refrigeración","7/12 °C","","Mín.","kW","0.75","1.15","1.32"]
["","","","Med.","kW","1.36","2.08","2.39"]
["","","","Máx.","kW","2.12","2.81","3.30"]
["Capacidad de refrigeración sensible","7/12 °C","","Mín.","kW","0.59","0.83","1.02"]
["","","","Med.","kW","1.04","1.51","1.84"]
["","","","Máx.","kW","1.54","2.11","2.65"]
["Capacidad de calefacción","45/40 °C","","Mín.","kW","0.82","1.20","1.47"]
["","","","Med.","kW","1.53","2.16","2.59"]
["","","","Máx.","kW","2.21","3.02","3.81"]
["Consumo","Mín.","","","kW","0","0.01","0.01"]
["","Med.","","","kW","0.01","0.01","0.01"]
["","Máx.","","","kW","0.02","0.02","0.03"]
["Velocidad del ventilador","Mín.","","","rpm","680.00","680.00","680.00"]
["","Med.","","","rpm","1100.00","1100.00","1100.00"]
["","Máx.","","","rpm","1500.00","1500.00","1500.00"]
["Carcasa","Color","","","","integrado","integrado","integrado"]
["","Material","","","","Sin carcasa","Sin carcasa","Sin carcasa"]
["Dimensiones","Unidad","","Altura","mm","576","576","576"]
["","","","Anchura","mm","725","925","1125"]
["","","","Profundidad","mm","126","126","126"]
["","Unidad con embalaje","","Altura","mm","690","690","690"]
["","","","Anchura","mm","830","1030","1230"]
["","","","Profundidad","mm","210","210","210"]
["Peso","Unidad","","","kg","12","15","18"]
["","Unidad con embalaje","","","kg","13","16","19"]
["Embalaje","Material","","","","Cartón","Cartón","Cartón"]
["","Peso","","","kg","1","1","1"]
["Intercambiador de calor","Cantidad","","","","1","1","1"]
["","Volumen interno de la batería","","","l","0.8","1.13","1.46"]
["","Carga","","Presión de funcionamiento","bar","10","10","10"]
["Circuito del agua","Diámetros de las conexiones de tuberías","","","in","3/4","3/4","3/4"]
["","Material de la tubería","","","","COBRE","COBRE","COBRE"]
["","Presión","Calefacción","Máx.","bar","10","10","10"]
["Circuito del agua, caída de presión del agua","Calefacción","45/40 °C","Mín.","kPa","1.50","2.70","3.00"]
["","","","Med.","kPa","4.30","9.30","8.90"]
["","","","Máx.","kPa","9.20","19.10","21.20"]
["","Refrigeración","7/12 °C","Mín.","kPa","1.90","2.70","2.50"]
["","","","Med.","kPa","4.30","9.90","8.80"]
["","","","Máx.","kPa","8.20","17.10","18.00"]
["Circuito del agua, caudal del agua","Calefacción","45/40 °C","Mín.","kg/h","140.00","210.00","260.00"]
["","","","Med.","kg/h","270.00","380.00","450.00"]
["","","","Máx.","kg/h","390.00","530.00","660.00"]
["","Refrigeración","7/12 °C","Mín.","kg/h","130.00","200.00","230.00"]
["","","","Med.","kg/h","230.00","360.00","410.00"]
["","","","Máx.","kg/h","360.00","480.00","570.00"]
["Nivel de potencia sonora","Mín.","","","dBA","35","36","36"]
["","Med.","","","dBA","45","46","47"]
["","Máx.","","","dBA","53.0","54.0","55.0"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","30","30","30"]
["","","","Máx.","°C","85","85","85"]
["","Refrigeración","Lado del agua","Mín.","°C","5","5","5"]
["","","","Máx.","°C","18","18","18"]
["","Instalación interior","Ambiente","Mín.","°CBS","0","0","0"]
["","","","Máx.","°CBS","45","45","45"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","No","No","No"]
["","Integrados en la unidad interior","","","","Sí","Sí","Sí"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Tensión","","","V","230","230","230"]
["Consumo eléctrico","Máx.","","","W","19","20","29"]
["","Espera","","","W","3","4","5"]
["Corriente","Corriente máxima de funcionamiento","","Calefacción","A","0.16","0.18","0.26"]
["","Corriente máx. de func.","","Refrigeración","A","0.16","0.18","0.26"]