{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":12,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Nivel de presión sonora","Calefacción","","A velocidad alta del ventilador","dBA","","","","","","48.0"]
["","","","A velocidad baja del ventilador","dBA","","","","","","45.0"]
["","","","A velocidad media del ventilador","dBA","","","","","","46.5"]
["","Refrigeración","","A velocidad baja del ventilador","dBA","","","","","","45.0"]
["","","","A velocidad alta del ventilador","dBA","","","","","","48.0"]
["","","","A velocidad media del ventilador","dBA","","","","","","46.5"]
["Accesorios estándar","Manual de instalación y de uso","","","","","","","","","1"]
["","Material de la abrazadera para cables","","","","","","","","","1"]
["","Arandela elástica","","","","","","","","","2"]
["","Tornillo hexagonal","","","","","","","","","2"]
["","Arandela plana","","","","","","","","","8"]
["","Tornillo hexagonal con arandela","","","","","","","","","49"]
["","Tubo de conexión del gas","","","","","","","","","1"]
["","Precauciones generales de seguridad","","","","","","","","","1"]
["Refrigerante","GWP","","","","","","","","","675"]
["","Tipo","","","","","","","","","R-32"]
["Consumo (50 Hz)","Refrigeración","","A velocidad alta del ventilador","kW","","","","","","0.54"]
["","Calefacción","","A velocidad alta del ventilador","kW","","","","","","0.54"]
["Capacidad de refrigeración","Capacidad total","","A velocidad alta del ventilador","kW","","","","","","22.4"]
["","Nom.","","","kW","","","","","","22.4"]
["Conexiones de tubería","Liquid","","OD","mm","","","","","","9.5"]
["","","","Tipo","","","","","","","Conexión abocardada"]
["","Gas","","D.E.","mm","","","","","","19.1"]
["","","","Tipo","","","","","","","Brida"]
["","Drain","","","","","","","","","BSP1"]
["Nivel de potencia sonora","Refrigeración","","A velocidad alta del ventilador","dBA","","","","","","75.0"]
["Dimensiones","Unidad","","Anchura","mm","","","","","","1,490"]
["","","","Profundidad","mm","","","","","","1,100"]
["","","","Altura","mm","","","","","","470"]
["Carcasa","Material","","","","","","","","","Placa de acero galvanizado"]
["","Color","","","","","","","","","Sin pintar"]
["Peso","Unidad","","","kg","","","","","","105"]
["Ventilador","Presión estática externa: 50Hz","","Alto","Pa","","","","","","250"]
["","","","Baja","Pa","","","","","","50"]
["","Presión estática externa: 60Hz","","Alto","Pa","","","","","","250"]
["","","","Baja","Pa","","","","","","50"]
["","Caudal de aire (50 Hz)","Refrigeración","A velocidad alta del ventilador","m³/min","","","","","","62"]
["","","","A velocidad baja del ventilador","m³/min","","","","","","41"]
["Capacidad de calefacción","Capacidad total","","A velocidad alta del ventilador","kW","","","","","","25.0"]
["","Nom.","","","kW","","","","","","25.0"]
["Corriente (50 Hz)","Amperios máximos del fusible (MFA)","","","A","","","","","","6"]
["Power supply","Fase","","","","","","","","","1~"]
["","Nombre","","","","","","","","","VM"]
["","Frecuencia","","","Hz","","","","","","50/60"]
["","Tensión","","","V","","","","","","220-240/220-230"]
["Capacidad de refrigeración","Capacidad total","","A velocidad alta del ventilador","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Capacidad de calefacción","Capacidad total","","A velocidad alta del ventilador","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Consumo - 50 Hz","Refrigeración","","A velocidad alta del ventilador","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Calefacción","","A velocidad alta del ventilador","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Dimensiones","Unidad","","Altura","mm","300","300","300","300","300","","470"]
["","","","Anchura","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Profundidad","mm","700","700","700","700","700","","1,100"]
["Peso","Unidad","","","kg","35","35","35","46","46","","115"]
["Carcasa","Color","","","","Sin pintar","Sin pintar","Sin pintar","Sin pintar","Sin pintar","","Sin pintar"]
["","Material","","","","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado","","Placa de acero galvanizado"]
["Espacio necesario en el falso techo >-=-mm","mm","","","","350","350","350","350","350"]
["Ventilador","Caudal de aire - 50Hz","Refrigeración","A velocidad alta del ventilador","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","A velocidad baja del ventilador","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","Presión estática externa: 50Hz","","Alto","Pa","200","200","200","200","200","","250"]
["","Presión estática externa: 60Hz","","Alto","Pa","200","200","200","200","200","","250"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","GWP","","","","675","675","675","675","675","","675"]
["Nivel de potencia sonora","Refrigeración","","A velocidad alta del ventilador","dBA","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Nivel de presión sonora","Refrigeración","","A velocidad alta del ventilador","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","A velocidad media del ventilador","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","A velocidad baja del ventilador","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Calefacción","","A velocidad alta del ventilador","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","A velocidad media del ventilador","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","A velocidad baja del ventilador","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Conexiones de tubería","Líquido","","Tipo","","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","","Conexión abocardada"]
["","","","D.E.","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Gas","","Tipo","","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","Conexión abocardada","","Brida"]
["","","","D.E.","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Drenaje","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Filtro de aire","Tipo","","","","Red de resina","Red de resina","Red de resina","Red de resina","Red de resina"]
["Accesorios estándar","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Alimentación eléctrica","Nombre","","","","VE","VE","VE","VE","VE","","VM"]
["","Fase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frecuencia","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["","Tensión","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Corriente - 50Hz","Amperios máximos del fusible (MFA)","","","A","6","6","6","6","6","","6"]
["Ventilador","Presión estática externa: 50Hz","","Baja","Pa","","","","","","","50"]
["","Presión estática externa: 60Hz","","Baja","Pa","","","","","","","50"]
["Accesorios estándar","General safety precautions","","","","","","","","","","1"]
["","Wire clamp material","","","","","","","","","","1"]
["","Spring washer","","","","","","","","","","2"]
["","Hexagon head screw","","","","","","","","","","2"]
["","Plain washer","","","","","","","","","","8"]
["","Hexagon head screw with washer","","","","","","","","","","49"]
["","Gas connection pipe","","","","","","","","","","1"]