{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-A"]
[]
[]
[]
[]
["","","","","","FXMQ200AXVMB","FXMQ250AXVMB"]
["Capacidad de refrigeración","Capacidad total","","A velocidad alta del ventilador","kW","22.4","28.0"]
["Capacidad de calefacción","Capacidad total","","A velocidad alta del ventilador","kW","25.0","31.5"]
["Consumo - 50 Hz","Refrigeración","","A velocidad alta del ventilador","kW","0.54","0.65"]
["","Calefacción","","A velocidad alta del ventilador","kW","0.54","0.65"]
["Dimensiones","Unidad","","Altura","mm","470","470"]
["","","","Anchura","mm","1490","1490"]
["","","","Profundidad","mm","1100","1100"]
["Peso","Unidad","","","kg","105","115"]
["Carcasa","Color","","","","Sin pintar","Sin pintar"]
["","Material","","","","Placa de acero galvanizado","Placa de acero galvanizado"]
["Ventilador","Caudal de aire - 50Hz","Refrigeración","A velocidad alta del ventilador","m³/min","62","74"]
["","","","A velocidad baja del ventilador","m³/min","41","52"]
["","Presión estática externa: 50Hz","","Alto","Pa","250","250"]
["","","","Baja","Pa","50","50"]
["","Presión estática externa: 60Hz","","Alto","Pa","250","250"]
["","","","Baja","Pa","50","50"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","GWP","","","","2087.5","2087.5"]
["Nivel de potencia sonora","Refrigeración","","A velocidad alta del ventilador","dBA","75.0","76.0"]
["Nivel de presión sonora","Refrigeración","","A velocidad alta del ventilador","dBA","48.0","48.0"]
["","","","A velocidad media del ventilador","dBA","46.5","46.5"]
["","","","A velocidad baja del ventilador","dBA","45.0","45.0"]
["","Calefacción","","A velocidad alta del ventilador","dBA","48.0","48.0"]
["","","","A velocidad media del ventilador","dBA","46.5","46.5"]
["","","","A velocidad baja del ventilador","dBA","45.0","45.0"]
["Conexiones de tubería","Líquido","","Tipo","","Conexión abocardada","Conexión abocardada"]
["","","","D.E.","mm","9.5","9.5"]
["","Gas","","Tipo","","Brida","Brida"]
["","","","D.E.","mm","19.1","22.2"]
["","Drenaje","","","","BSP1","BSP1"]
["Accesorios estándar","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","1","1"]
["","Spring washer","","","","2","2"]
["","Hexagon head screw","","","","2","2"]
["","Plain washer","","","","8","8"]
["","Hexagon head screw with washer","","","","49","49"]
["","Gas connection pipe","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["Alimentación eléctrica","Nombre","","","","VM","VM"]
["","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50/60","50/60"]
["","Tensión","","","V","220-240/220-230","220-240/220-230"]
["Corriente - 50Hz","Amperios máximos del fusible (MFA)","","","A","6","6"]