{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":5,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-P7H"]
[]
[]
[]
[]
["","","","","FXMQ50P7VEH"]
["Refrigerante","Tipo","","","R-410A"]
["Capacidad de refrigeración","Nom.","","kW","5.6 (1)"]
["Piping connections","Líquido","D.E.","mm","6.35"]
["","","Tipo","","Conexión abocardada"]
["","Gas","D.E.","mm","12.7"]
["","","Tipo","","Conexión abocardada"]
["","Drenaje","","","VP25 (I.D. 25/O.D. 32)"]
["Espacio necesario en el falso techo >","mm","","","350"]
["Dimensiones","Unidad","Anchura","mm","1,000"]
["","","Profundidad","mm","700"]
["","","Altura","mm","300"]
["Carcasa","Material","","","Placa de acero galvanizado"]
["","Colour","","","Sin pintar"]
["Peso","Unidad","","kg","35"]
["Ventilador","Presión estática externa: 60Hz","Alto","Pa","200"]
["Altura de drenaje","mm","","","625"]
["Panel decorativo","Peso","","kg","4.5"]
["","Modelo","","","BYBS71DJW1"]
["","Dimensiones","Altura","mm","55"]
["","","Profundidad","mm","500"]
["","","Anchura","mm","1,100"]
["","Color","","","Blanco (10Y9/0,5)"]
["Capacidad de calefacción","Nom.","","kW","6.3 (2)"]
["Power supply","Fase","","","1~"]
["","Frecuencia","","Hz","50/60"]
["","Nombre","","","VE"]
["","Tensión","","V","220-240/220 +/-10%"]
["Notas","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m"]