{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LREN-A / LRNUN-AY1"]
[]
[]
[]
[]
["","","","","LREN12AY1B / LRNUN5AY1"]
["Capacidad de refrigeración","Temperatura media","kW","kW","31.7 (4)"]
["","Temperatura baja","kW","kW","17.3 (3)"]
["Consumo","Temperatura media","Nom.","kW","20.1 (4)"]
["","Temperatura baja","Nom.","kW","18.6 (3)"]
["COP","Temperatura media","Nom.","","1.58 (4)"]
["","Temperatura baja","Nom.","","0.93 (3)"]
["Notas","","","","(1) - Minimum load of each individual refrigeration indoor unit: 3 KW (for Medium Temperature Operation)"]
["","","","","(2) - Minimum load of each individual refrigeration indoor unit: 2 KW (for Low Temperature Operation)."]
["","","","","(3) - Condiciones nominales: temperatura de saturación equivalente a la presión de aspiración: -35 °C (LT), temp. exterior 32 °C, aspiración SH 10K."]
["","","","","(4) - Rated conditions: saturation temperature equivalent to suction pressure: -10°C (MT), outdoor temp. 32°C, Suction SH 10K"]
["","","","","(5) - Sound pressure data: measured at 1m in front of unit, at 1.5m height. Nominal operation condition – Medium evaporation temperature (MT)"]
["","","","","(6) - For MT (Medium Temperature) Operation"]
["","","","","(7) - For LT (Low Temperature) Operation"]