{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Accesorios estándar","Declaración de conformidad","","","","1"]
["Peso","Unidad","","","kg","173"]
["Refrigerante","GWP","","","","1.0"]
["","Carga","","","kg","3.20"]
["Motor del ventilador","Potencia","","","W","350"]
["Intercambiador de calor","Tipo","","","","Batería de aletas cruzadas"]
["Dimensiones","Unidad","","Anchura","mm","635"]
["","","","Profundidad","mm","765"]
["","","","Altura","mm","1,680"]
["Carcasa","Color","","","","Blanco marfil"]
["Ventilador","Tipo","","","","Ventilador helicoidal"]
["","Caudal de aire","Refrigeración","Nom.","m³/min","102"]
["","Cantidad","","","","1"]
["Power supply","Fase","","","","3N~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","380-415"]
["Notas","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Compresor 1"]
["","","","","","(3) - Compresor 2"]
["","","","","","(4) - Compresor 3"]
["","","","","","(5) - Carga de la unidad de fábrica"]
["","","","","","(6) - Solo se permite utilizar K65 con un D.P. de 120 bar en conexiones de tubería AC."]
["","","","","","(7) - La presión de la válvula de seguridad se muestra como la presión manométrica."]
["","","","","","(8) - Solo se permite utilizar K65 con una D.P. de 90 bar en conexiones de tubería AC."]