{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEN-AY1"]
[]
[]
[]
[]
["","","","","","LRYEN10A7Y1"]
["Carcasa","Color","","","","Blanco marfil"]
["Dimensiones","Unidad","","Altura","mm","1680"]
["","","","Anchura","mm","1930"]
["","","","Profundidad","mm","765"]
["Peso","Unidad","","","kg","563"]
["Ventilador","Tipo","","","","Ventilador helicoidal"]
["","Cantidad","","","","3"]
["","Caudal de aire","Refrigeración","Nom.","m³/min","300"]
["Motor del ventilador","Potencia","","","W","750"]
["Intercambiador de calor","Tipo","","","","Batería de aletas cruzadas"]
["Refrigerante","Tipo 2","","","","R-744"]
["","GWP","","","","1.0"]
["","Carga","","","kg","6.30"]
["Accesorios estándar","Installation manual","","","","1"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Copper packing for stop valve (15 pcs)","","","","1"]
["","Copper packing for service port (15 pcs)","","","","1"]
["","Declaration of conformity","","","","1"]
["Alimentación eléctrica","Fase","","","","3N~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","380-415"]
["Notas","","","","","(1) - Compresor 1"]
["","","","","","(2) - Compresor 2"]
["","","","","","(3) - Compresor 3"]
["","","","","","(4) - Carga de la unidad de fábrica"]