{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Tipo","","","","","Purificador de aire humidificador"]
["Aplicación","","","","","Unidad de suelo"]
["Carcasa","Color","","","","Blanco (N9. 0)"]
["Dimensiones","Unidad","","Altura","mm","600 (5)"]
["","","","Anchura","mm","395"]
["","","","Profundidad","mm","287"]
["Peso","Unidad","","","kg","12.5"]
["Superficie máxima de la estancia","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Operación de purificación de aire","Consumo","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","B","kW","0.01"]
["","","","Funcionamiento silencioso","kW","0.008"]
["Función de humidificación","Consumo","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","B","kW","0.012"]
["","","","Funcionamiento silencioso","kW","0.011"]
["","Capacidad del depósito de agua","","","l","3.6"]
["Nivel de presión sonora","Operación de purificación de aire","","Turbo","dBA","54"]
["","","","Media","dBA","37"]
["","","","Bajo","dBA","27"]
["","","","Funcionamiento silencioso","dBA","18"]
["","Función de humidificación","","Turbo","dBA","54"]
["","","","Medio","dBA","37"]
["","","","Bajo","dBA","27"]
["","","","Funcionamiento silencioso","dBA","23"]
["Ventilador","Caudal de aire","Operación de purificación de aire","Turbo","m³/h","420"]
["","","","Medio","m³/h","210"]
["","","","Bajo","m³/h","132"]
["","","","Funcionamiento silencioso","m³/h","60"]
["","","Función de humidificación","Turbo","m³/h","420"]
["","","","Medio","m³/h","210"]
["","","","Bajo","m³/h","132"]
["","","","Funcionamiento silencioso","m³/h","102"]
["Método de captación de polvo","","","","","Filtro HEPA electrostático"]
["Método desodorizante","","","","","Flash Streamer + Catalizador desodorizante"]
["Accesorios estándar","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Cable de alimentación eléctrica","m","","","","2"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50/60"]
["","Tensión","","","V","220-240/220-230"]
["Notas","","","","","(1) - El área de cobertura es adecuada para operar la unidad a la máxima velocidad del ventilador (HH). El área de cobertura indica el espacio donde una cierta cantidad de partículas de polvo puede eliminarse en 30 minutos"]
["","","","","","(2) - Conversión a estándares NRCC a partir de valores de prueba conforme a JEM1467."]
["","","","","","(3) - Los niveles de sonido de funcionamiento son el promedio de los valores medidos a 1 m de distancia de la parte delantera, izquierda, derecha y superior de la unidad. (Estos son equivalentes a los valores en una cámara anecoica)"]