{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-KM"]
[]
[]
[]
[]
["","","","","","RX25KMV1B","RX35KMV1B"]
["Dimensiones","Unidad","","Altura","mm","550","550"]
["","","","Anchura","mm","675","675"]
["","","","Profundidad","mm","284","284"]
["Peso","Unidad","","","kg","24","28"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","10 (1)","10 (1)"]
["","","","Máx.","°CBS","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15"]
["","","","Máx.","°CBH","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46","48"]
["","Calefacción","","Alto","dBA","47","48"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","Carga","","","kg","0.70","0.94"]
["","Carga","","","tCO2Eq","1.5","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","15","15"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","12","12"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug (only heat pump models)","","","","1","1"]
["","Drain cap","","","","6","6"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]
["Notas","","","","","(1) - Límites de func. con FTX-J3: mín. 10°CBS ~ máx. 46°CBS","(1) - Límites de func. con FTX-J3: mín. 10°CBS ~ máx. 46°CBS"]