{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA50B2V1B","RXA50B5V1B"]
["Dimensiones","Unidad","","Altura","mm","734","734","734"]
["","","","Anchura","mm","870","870","954"]
["","","","Profundidad","mm","373","373","401"]
["Peso","Unidad","","","kg","50","50","49"]
["Compressor","Type","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10","-10"]
["","","","Máx.","°CBS","46","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15","-15"]
["","","","Máx.","°CBH","18","18","18"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","48.0","48.0","48"]
["","Calefacción","","Nom.","dBA","48.0","48.0","48"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32"]
["","Carga","","","kg","1.10","1.10","1.1"]
["","Carga","","","tCO2Eq","0.75","0.75","0.75"]
["","GWP","","","","675","675","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","30","30","30"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","20","20","20"]
["Accesorios estándar","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240"]
["Compresor","Tipo","","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Notas","","","","","","","(1) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","","","(2) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","","","","(3) - Contiene gases fluorados de efecto invernadero"]