{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-F"]
[]
[]
[]
[]
["","","","","","RXF20F5V1B","RXF25F5V1B","RXF35F5V1B","RXF42F5V1B","RXF50F5V1B"]
["Dimensiones","Unidad","","Altura","mm","556","556","556","556","610"]
["","","","Anchura","mm","740","740","740","740","923"]
["","","","Profundidad","mm","343","343","343","343","367"]
["Peso","Unidad","","","kg","24.0","24.0","24.0","28.0","40.0"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10","-10","-10","-10"]
["","","","Máx.","°CBS","48","48","48","48","48"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15","-15","-15","-15"]
["","","","Máx.","°CBH","18","18","18","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46.0","46.0","48.0","48.0","48.0"]
["","Calefacción","","Alto","dBA","47.0","47.0","48.0","48.0","49.0"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.420","0.420","0.500","0.750","0.800"]
["","Carga","","","tCO2Eq","0.280","0.280","0.340","0.510","0.540"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20","20","20","30"]
["","Carga de refrigerante adicional.","","","kg/m","002 (para longitud de tubería superior a 10 m)","002 (para longitud de tubería superior a 10 m)","002 (para longitud de tubería superior a 10 m)","002 (para longitud de tubería superior a 10 m)","002 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","12.0","12.0","12.0","12.0","20.0"]
["Accesorios estándar","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero","(1) - Contiene gases fluorados de efecto invernadero"]
["","","","","","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]