{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M2V1B","RXJ20M3V1B","RXJ20M5V1B","RXJ25M2V1B","RXJ25M3V1B","RXJ25M5V1B","RXJ35M2V1B","RXJ35M3V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","29.3","","","29.3","","","29.3","","","38.5"]
["","","Calefacción","Súper baja","m³/min","25.6","","","25.6","","","25.6","","","34.3"]
["","","","Súper baja","cfm","1035","","","1035","","","1035","","","1359"]
["","","Calefacción","Súper baja","cfm","904","","","904","","","904","","","1211"]
["Dimensiones","Unidad","","Altura","mm","550","550","550","550","550","550","550","550","550","735","735"]
["","","","Anchura","mm","765","765","765","765","765","765","765","765","765","825","825"]
["","","","Profundidad","mm","285","285","285","285","285","285","285","285","285","300","300"]
["Peso","Unidad","","","kg","34","32","32","34","32","32","34","32","32","44","44"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","760","","","760","","","760","","","620"]
["","","Calefacción","Súper baja","rpm","740","","","740","","","740","","","620"]
["Compressor","Type","","","","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Máx.","°CBS","46","46","46","46","46","46","46","46","46","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Máx.","°CBH","18","18","18","18","18","18","18","18","18","18","20"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46","","","46","","","48","","","48","48"]
["","","","Nom.","dBA","","46","46","","46","46","","49","49"]
["","","","Bajo","dBA","","","","","","","","","","","45"]
["","Calefacción","","Alto","dBA","47","","","47","","","48","","","48","48"]
["","","","Nom.","dBA","","47","47","","47","47","","49","49"]
["","","","Bajo","dBA","","","","","","","","","","","45"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76","1.30","1.3"]
["","Carga","","","tCO2Eq","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52","0.9","0.88"]
["","GWP","","","","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0","675","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20","20","20","20","20","20","20","20","30","30"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0","20"]
["Accesorios estándar","Installation manual","","","","1","1","","1","1","","1","1","","1"]
["","Drain plug","","","","1","1","","1","1","","1","1","","1"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - 220 V","","","(1) - 220 V","","","(1) - 220 V","","","(1) - 220 V"]
["","","","","","(2) - 230V","","","(2) - 230V","","","(2) - 230V","","","(2) - 230V"]
["","","","","","(3) - 240V","","","(3) - 240V","","","(3) - 240V","","","(3) - 240V"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Accesorios estándar","Refrigerant charge label","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","1","","","1","","","1"]