{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","30.6","30.6"]
["","","Calefacción","Súper baja","m³/min","27.2","27.2"]
["","","","Súper baja","cfm","1080","1080"]
["","","Calefacción","Súper baja","cfm","960","960"]
["Dimensiones","Unidad","","Altura","mm","550","550"]
["","","","Anchura","mm","858","858"]
["","","","Profundidad","mm","330","330"]
["Peso","Unidad","","","kg","40","40"]
["Compresor","Type","","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10"]
["","","","Máx.","°CBS","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-25","-25"]
["","","","Máx.","°CBH","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","48","48"]
["","","","Bajo","dBA","44","44"]
["","Calefacción","","Alto","dBA","49","49"]
["","","","Bajo","dBA","45","45"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","Carga","","","kg","1","1"]
["","Carga","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. int.","Máx.","m","15","15"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado"]