{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-R"]
[]
[]
[]
[]
["","","","","","RXM20R5V1B","RXM25R5V1B","RXM35R5V1B","RXM42R2V1B","RXM42R5V1B","RXM50R2V1B","RXM50R5V1B","RXM60R2V1B","RXM60R5V1B","RXM71R2V1B"]
["Dimensiones","Unidad","","Altura","mm","552","552","552","734","734","734","734","734","734","734"]
["","","","Anchura","mm","840","840","840","954","954","954","954","954","954","954"]
["","","","Profundidad","mm","350","350","350","401","401","401","401","401","401","401"]
["Peso","Unidad","","","kg","32","32","32","49.0","49.0","49.0","49.0","49.0","49.0","55"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Máx.","°CBS","50 (4), 46 (5)","50 (4), 46 (5)","50 (4), 46 (5)","50, 46","50, 46","50, 46","50, 46","50, 46","50, 46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15","-15","-15","-21","-15","-21","-15","-21","-15"]
["","","","Máx.","°CBH","18","18","18","18","18","18","18","18","18","18"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","46","46","49","48.0","48.0","48.0","48.0","48.0","48.0","47.0"]
["","Calefacción","","Nom.","dBA","47","47","49","48.0","48.0","49.0","49.0","49.0","49.0","48.0"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.76","0.76","0.76","1.10","1.10","1.15","1.15","1.15","1.15","1.15"]
["","Carga","","","tCO2Eq","0.52","0.52","0.52","0.750","0.750","0.780","0.780","0.780","0.780","0.780"]
["","GWP","","","","675","675","675","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20","20","30","30","30","30","30","30","30"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","15","15","20.0","20.0","20.0","20.0","20.0","20.0","20.0"]
["Accesorios estándar","Installation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - Solo posible en combinación con CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Solo posible en combinación con CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Solo posible en combinación con CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B"]
["","","","","","(2) - Solo posible en combinación con CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·","(2) - Solo posible en combinación con CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·","(2) - Solo posible en combinación con CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·"]
["Accesorios estándar","Drain cap","","","","","","","3","3","3","3","3","3","3"]