{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":11,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","47","47","48","48"]
["","Refrigeración","","Alto","dBA","46","46","48","48"]
["Accesorios estándar","Tapón de drenaje","","","","1","1","1","1"]
["","Manual de instalación","","","","1","1","1","1"]
["","Etiqueta de carga de refrigerante","","","","1","1","1"]
["","Etiquetas multilingües para gases de efecto invernadero fluorados","","","","1","1","Etiquetas multilingües para gases de efecto invernadero fluorados"]
["Refrigerante","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Carga","","","kg","1.0","1.0","1.20","1.3"]
["","Tipo","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","780","780","780","790"]
["","","Calefacción","Súper baja","rpm","740","740","740","780"]
["Límites de funcionamiento","Refrigeración","Ambiente","Máx.","°CBS","46","46","46","46"]
["","","","Mín.","°CBS","-10","-10","-10","-10"]
["","Calefacción","Ambiente","Máx.","°CBH","18","18","18","18"]
["","","","Mín.","°CBH","-15","-15","-15","-15"]
["Piping connections","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","","15"]
["","Carga de refrigerante adicional.","","","kg/m","","","0,020 (para longitud de tubería superior a 10 m)"]
["Dimensiones","Unidad","","Anchura","mm","765","765","765","765"]
["","","","Profundidad","mm","285","285","285","285"]
["","","","Altura","mm","550","550","550","550"]
["Compresor","Type","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Peso","Unidad","","","kg","34","34","34","39"]
["Ventilador","Caudal de aire","Calefacción","Súper baja","cfm","904","904","904","960"]
["","","","Súper baja","m³/min","25.6","25.6","25.6","27.2"]
["","","Refrigeración","Súper baja","m³/min","30.1","30.1","30.1","30.6"]
["","","","Súper baja","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Contiene gases fluorados de efecto invernadero","(4) - Contiene gases fluorados de efecto invernadero","(4) - Contiene gases fluorados de efecto invernadero","(4) - Contiene gases fluorados de efecto invernadero"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","","","","","48.9","45.0"]
["","","Calefacción","Súper baja","m³/min","","","","","43.1","46.3"]
["","","","Súper baja","cfm","","","","","1727","1589"]
["","","Calefacción","Súper baja","cfm","","","","","1522","1635"]
["Dimensiones","Unidad","","Altura","mm","","","","","735","735"]
["","","","Anchura","mm","","","","","825","825"]
["","","","Profundidad","mm","","","","","300","300"]
["Peso","Unidad","","","kg","","","","","47","48"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","","","","","670"]
["","","Calefacción","Súper baja","rpm","","","","","670"]
["Compresor","Tipo","","","","","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","","","","","-10","-10"]
["","","","Máx.","°CBS","","","","","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","","","","","-15","-15"]
["","","","Máx.","°CBH","","","","","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","","","","48","49"]
["","","","Bajo","dBA","","","","","44","46"]
["","Calefacción","","Alto","dBA","","","","","48","49"]
["","","","Bajo","dBA","","","","","45","46"]
["Refrigerante","Tipo","","","","","","","","R-410A","R-410A"]
["","Carga","","","kg","","","","","1.7","1.5"]
["","Carga","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","","","","","30","30"]
["","Carga de refrigerante adicional.","","","kg/m","","","","","0,020 (para longitud de tubería superior a 10 m)","0,020 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","","","","20.0","20"]
["Accesorios estándar","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Alimentación eléctrica","Fase","","","","","","","","1~","1~"]
["","Frecuencia","","","Hz","","","","","50","50"]
["","Tensión","","","V","","","","","220-230-240","220-230-240"]
["Notas","","","","","","","","","","(1) - 230V"]