{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","","48"]
["","Refrigeración","","Alto","dBA","","","48"]
["Accesorios estándar","Manual de instalación","","","","","","1"]
["","Etiqueta de carga de refrigerante","","","","","","1"]
["","Etiquetas multilingües para gases de efecto invernadero fluorados","","","","","","1"]
["","Tapón de drenaje (solo modelos con bomba de calor)","","","","","","1"]
["Refrigerante","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Carga","","","kg","","","1.2"]
["","Tipo","","","","","","R-410A"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","","","780"]
["","","Calefacción","Súper baja","rpm","","","740"]
["Límites de funcionamiento","Refrigeración","Ambiente","Máx.","°CBS","","","46"]
["","","","Mín.","°CBS","","","-10"]
["","Calefacción","Ambiente","Máx.","°CBH","","","18"]
["","","","Mín.","°CBH","","","-15"]
["Piping connections","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","","15"]
["","Carga de refrigerante adicional.","","","kg/m","","","0,02 (para longitud de tubería superior a 10 m)"]
["Dimensiones","Unidad","","Anchura","mm","","","765"]
["","","","Profundidad","mm","","","285"]
["","","","Altura","mm","","","550"]
["Compresor","Type","","","","","","Compresor swing herméticamente sellado"]
["Peso","Unidad","","","kg","","","34"]
["Ventilador","Caudal de aire","Calefacción","Súper baja","cfm","","","904"]
["","","","Súper baja","m³/min","","","25.6"]
["","","Refrigeración","Súper baja","m³/min","","","30.1"]
["","","","Súper baja","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Frecuencia","","","Hz","","","50"]
["","Tensión","","","V","","","220-240"]
["Notas","","","","","","","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire."]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","30.1","30.1"]
["","","Calefacción","Súper baja","m³/min","25.6","25.6"]
["","","","Súper baja","cfm","1063","1063"]
["","","Calefacción","Súper baja","cfm","904","904"]
["Dimensiones","Unidad","","Altura","mm","550","550"]
["","","","Anchura","mm","765","765"]
["","","","Profundidad","mm","285","285"]
["Peso","Unidad","","","kg","34","34"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","780","780"]
["","","Calefacción","Súper baja","rpm","740","740"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10"]
["","","","Máx.","°CBS","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15"]
["","","","Máx.","°CBH","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46","46"]
["","Calefacción","","Alto","dBA","47","47"]
["Refrigerante","Tipo","","","","R-410A","R-410A"]
["","Carga","","","kg","1.0","1.0"]
["","Carga","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","15"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]
["Notas","","","","","(1) - 220 V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Accesorios estándar","Drain plug (only heat pump models)","","","","","1"]