{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","","48","48","50","50"]
["","Refrigeración","","Alto","dBA","","","48","48","49","49"]
["Accesorios estándar","Manual de uso","","","","","","1","1","1","1"]
["","Manual de instalación","","","","","","1","1","1","1"]
["Refrigerante","GWP","","","","","","675","675","675","675"]
["","Carga","","","kg","","","1.34","1.34","1.34","1.34"]
["","Tipo","","","","","","R-32","R-32","R-32","R-32"]
["Rango de funcionamiento","Refrigeración","Ambiente","Máx.","°CBS","","","43","43","43","43"]
["","","","Mín.","°CBS","","","-10","-10","-10","-10"]
["","Calefacción","Ambiente","Máx.","°CBH","","","18","18","18","18"]
["","","","Mín.","°CBH","","","-20","-20","-20","-20"]
["Conexiones de tubería","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","","8","8","8","8"]
["Dimensiones","Unidad","","Anchura","mm","","","795","795","795","795"]
["","","","Profundidad","mm","","","300","300","300","300"]
["","","","Altura","mm","","","693","693","693","693"]
["Compresor","Tipo","","","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Peso","Unidad","","","kg","","","50","50","50","50"]
["Power supply","Fase","","","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","","","50","50","50","50"]
["","Tensión","","","V","","","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Contiene gases fluorados de efecto invernadero","(4) - Contiene gases fluorados de efecto invernadero","(4) - Contiene gases fluorados de efecto invernadero","(4) - Contiene gases fluorados de efecto invernadero"]
["Dimensiones","Unidad","","Altura","mm","693","693"]
["","","","Anchura","mm","795","795"]
["","","","Profundidad","mm","300","300"]
["Peso","Unidad","","","kg","50","50"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10"]
["","","","Máx.","°CBS","43","43"]
["","Calefacción","Ambiente","Mín.","°CBH","-20","-20"]
["","","","Máx.","°CBH","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46","46"]
["","Calefacción","","Alto","dBA","46","46"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","1.34","1.34"]
["","Carga","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","10","10"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","8","8"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]