{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensiones","Unidad","","Altura","mm","870","870"]
["","","","Anchura","mm","1,100","1,100"]
["","","","Profundidad","mm","460","460"]
["Peso","Unidad","","","kg","117","117"]
["Compresor","Type","","","","Compresor scroll herméticamente sellado","Compresor scroll herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-20","-20"]
["","","","Máx.","°CBS","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-20","-20"]
["","","","Máx.","°CBH","15","15"]
["Nivel de potencia sonora","Refrigeración","","","dBA","73","76"]
["","Calefacción","","","dBA","76 (1)","79 (1)"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","53","57"]
["","Calefacción","","Nom.","dBA","60","63"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","5","5"]
["","GWP","","","","675","675"]
["Piping connections","Liquid","","OD","mm","9.52","9.52"]
["","Gas","","D.E.","mm","22.2","22.2"]
["","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","100","100"]
["","","Sistema","Sin carga","m","30","30"]
["","Carga de refrigerante adicional.","","","kg/m","Consulte el manual de instalación","Consulte el manual de instalación"]
["Accesorios estándar","Manual de instalación","","","","1","1"]
["","Precauciones generales de seguridad","","","","1","1"]
["","Arrollamientos de unión","","","","2","2"]
["","Quite la etiqueta de gases fluorados","","","","1","1"]
["","Tubos de conexión","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","380-415","380-415"]
["Corriente (50 Hz)","Amperios máximos del fusible (MFA)","","","A","20","20"]
["Notas","","","","","(1) - Según ENER Lot 21","(1) - Según ENER Lot 21"]