{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Dimensiones","Unidad","","Altura","mm","734","734","734"]
["","","","Anchura","mm","870","870","870"]
["","","","Profundidad","mm","373","373","373"]
["Peso","Unidad","","","kg","52","52","52"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-20","-20","-20"]
["","","","Máx.","°CBS","52","52","52"]
["","Calefacción","Ambiente","Mín.","°CBH","-21","-21","-21"]
["","","","Máx.","°CBH","18","18","18"]
["Nivel de potencia sonora","Refrigeración","","","dBA","62","63","64"]
["","Calefacción","","","dBA","62","63","64"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","48","49","50"]
["","Calefacción","","Nom.","dBA","48","49","50"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32"]
["","Carga","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Carga","","","tCO2Eq","1.05","1.05","1.05"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.52","12.7","12.7"]
["","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","50","50","50"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)","0,02 (para longitud de tubería superior a 30 m)","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","30","30","30"]
["Accesorios estándar","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240"]
["Notas","","","","","(1) - Consulte la ilustración por separado para el rango de funcionamiento","(1) - Consulte la ilustración por separado para el rango de funcionamiento","(1) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos.","(2) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","","(3) - Contiene gases fluorados de efecto invernadero","(3) - Contiene gases fluorados de efecto invernadero","(3) - Contiene gases fluorados de efecto invernadero"]
["Accesorios estándar","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]