{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NV1"]
[]
[]
[]
[]
["","","","","","RZAG71N7V1B","RZAG71N2V1B","RZAG100N7V1B","RZAG100N2V1B","RZAG125N7V1B","RZAG125N2V1B","RZAG140N7V1B","RZAG140N2V1B"]
["Dimensiones","Unidad","","Altura","mm","870","870","870","870","870","870","870","870"]
["","","","Anchura","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Profundidad","mm","460","460","460","460","460","460","460","460"]
["Peso","Unidad","","","kg","81","81","85","85","95","95","95","95"]
["Compressor","Tipo","","","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Máx.","°CBS","52","52","52","52","52","52","52","52"]
["","Calefacción","Ambiente","Mín.","°CBH","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Máx.","°CBH","18","18","18","18","18","18","18","18"]
["Nivel de potencia sonora","Refrigeración","","","dBA","64","64","66","66","69","69","70","70"]
["","Calefacción","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Calefacción","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","3.2","3.20","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["","Carga","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Conexiones de tubería","Líquido","","D.E.","mm","10","10","10","10","10","10","10","10"]
["","Gas","","D.E.","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","55","55","85","85","85","85","85","85"]
["","","Sistema","Equivalente","m","75","75","100","100","100","100","100","100"]
["","","","Sin carga","m","40","40","40","40","40","40","40","40"]
["","Carga de refrigerante adicional.","","","kg/m","Consulte el manual de instalación","Consulte el manual de instalación","Consulte el manual de instalación","Consulte el manual de instalación","Consulte el manual de instalación","Consulte el manual de instalación","Consulte el manual de instalación","Consulte el manual de instalación"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","30","30","30","30","30","30","30","30"]
["","","Ud. int. – Ud. int.","Máx.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Accesorios estándar","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Corriente - 50Hz","Amperios máximos del fusible (MFA)","","","A","20","20","32","32","32","32","32","32"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Notas","","","","","","","","","(1) - Según ENER Lot 21","(1) - Según ENER Lot 21","(1) - Según ENER Lot 21","(1) - Según ENER Lot 21"]