{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensiones","Unidad","","Altura","mm","1,680"]
["","","","Anchura","mm","930"]
["","","","Profundidad","mm","765"]
["Peso","Unidad","","","kg","183.0"]
["Compressor","Type","","","","Compresor scroll herméticamente sellado"]
["Rango de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-5.0"]
["","","","Máx.","°CBS","46.0"]
["","Heating","Ambiente","Mín.","°CBH","-15.0"]
["","","","Máx.","°CBH","15.0"]
["Sound power level","Refrigeración","","","dBA","78.0"]
["","Calefacción","","","dBA","78.0"]
["Refrigerante","Tipo","","","","R-410A"]
["","Carga","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Conexiones de tubería","Líquido","","D.E.","mm","9.52"]
["","Gas","","D.E.","mm","22.2"]
["","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","100"]
["","","Sistema","Sin carga","m","30"]
["Accesorios estándar","Manual de instalación","","","","1"]
["","Tubos de conexión","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","380-415"]
["Corriente (50 Hz)","Amperios máximos del fusible (MFA)","","","A","25"]
["Notas","","","","","(1) - La alimentación eléctrica de las unidades interiores FDQ es independiente."]
["","","","","","(2) - Consulte los planos independientes con los datos eléctricos."]
["Dimensiones","Unidad","","Altura","mm","","1680"]
["","","","Anchura","mm","","930"]
["","","","Profundidad","mm","","765"]
["Peso","Unidad","","","kg","","184.0"]
["Compresor","Tipo","","","","","Compresor scroll herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","","-5.0"]
["","","","Máx.","°CBS","","46.0"]
["","Calefacción","Ambiente","Mín.","°CBH","","-15.0"]
["","","","Máx.","°CBH","","15.0"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","78.0"]
["","Calefacción","","","dBA","","78.0"]
["Refrigerante","Carga","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Carga","","","tCO2Eq","","19.4"]
["Conexiones de tubería","Líquido","","D.E.","mm","","12.70"]
["","Gas","","D.E.","mm","","22.2"]
["","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","","100"]
["","","Sistema","Sin carga","m","","30"]
["Accesorios estándar","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Alimentación eléctrica","Frecuencia","","","Hz","","50"]
["Corriente - 50Hz","Amperios máximos del fusible (MFA)","","","A","","25"]