{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":10,"n_cols":16,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ALB-RBS"]
[]
[]
[]
[]
["","","","","ALB02RBSNADBT01","ALB03RBSNADBT01","ALB04RBSNADBT01","ALB05RBSNADBT01","ALB06RBSNADBT01","ALB07RBSNADBT01","ALB02RBSNADBT00 (Archived)","ALB03RBSNADBT00 (Archived)","ALB04RBSNADBT00 (Archived)","ALB05RBSNADBT00 (Archived)","ALB06RBSNADBT00 (Archived)","ALB07RBSNADBT00 (Archived)"]
["Dimensiones","Unidad","Anchura","mm","920","1,100","1,600","1,600","2,000","2,000","920","1,100","1,600","1,600","2,000","2,000"]
["Ventilador de retorno","Tensión","","","200-277","200-277","200-277","200-277","200-277","200-277","200-277","200-277","200-277","200-277","200-277","200-277"]
["","Frecuencia","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Potencia","","kW","0.06","0.15","0.25","0.32","2x0.26","2x0.37","0.06","0.14","0.24","0.3","2x0.23","2x0.31"]