{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Consumo","Refrigeración","","Nom.","kW","0.020"]
["","Calefacción","","Nom.","kW","0.020"]
["Carcasa","Color","","","","Negro"]
["Dimensiones","Unidad","","Altura","mm","295"]
["","","","Anchura","mm","798"]
["","","","Profundidad","mm","189"]
["Peso","Unidad","","","kg","11.5"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","11.0"]
["","","","Medio","m³/min","8.2"]
["","","","Bajo","m³/min","6.1"]
["","","","Funcionamiento silencioso","m³/min","4.6"]
["","","Calefacción","Alto","m³/min","10.9"]
["","","","Medio","m³/min","8.7"]
["","","","Bajo","m³/min","6.4"]
["","","","Funcionamiento silencioso","m³/min","4.5"]
["Sound power level","Refrigeración","","","dBA","57"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","39"]
["","","","Medio","dBA","32"]
["","","","Bajo","dBA","25"]
["","","","Funcionamiento silencioso","dBA","21"]
["","Calefacción","","Alto","dBA","39"]
["","","","Medio","dBA","32"]
["","","","Bajo","dBA","25"]
["","","","Funcionamiento silencioso","dBA","21"]
["Refrigerante","GWP","","","","675.0"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35"]
["","Gas","","D.E.","mm","9.50"]
["","Drain","","","","18"]
["Sistemas de control","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Accesorios estándar","Manual de instalación","","","","1"]
["","Manual de uso","","","","1"]
["","Filtro de aire","","","","2"]
["","Mando a distancia por infrarrojos","","","","1"]
["","Placa de instalación del mando a distancia","","","","1"]
["","Bolsa de tornillos","","","","1"]
["","Cubierta roscada","","","","2"]
["","Pilas secas AAA","","","","2"]
["","Precauciones generales de seguridad","","","","1"]
["Power supply","Nombre","","","","V1"]
["","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]