{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Nivel de presión sonora","Calefacción","Alto","dBA","38"]
["","","Medio","dBA","36"]
["","","Bajo","dBA","30"]
["","Refrigeración","Medio","dBA","36"]
["","","Bajo","dBA","30"]
["","","Alto","dBA","38"]
["Accesorios estándar","Manual de instalación","","","1"]
["","Manual de uso","","","1"]
["","Aislamiento para adaptador","","","1"]
["","Almohadilla de sellado","","","1"]
["","Abrazadera metálica","","","1"]
["","Tubo flexible de drenaje","","","1"]
["","Arandela para ménsula de suspensión","","","8"]
["","Material de sellado","","","2"]
["","Abrazaderas","","","6"]
["","Arandela para placa de fijación","","","4"]
["","Tornillos para bridas de conducto","","","1"]
["","Filtro de aire","","","1"]
["Conexiones de tubería","Liquid","OD","mm","6.35"]
["","Gas","D.E.","mm","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Refrigeración","Nom.","kW","0.060"]
["","Calefacción","Nom.","kW","0.060"]
["Sound power level","Refrigeración","","dBA","55"]
["","Calefacción","","dBA","55"]
["Dimensiones","Unidad","Anchura","mm","1,150"]
["","","Profundidad","mm","620"]
["","","Altura","mm","200"]
["Peso","Unidad","","kg","30.0"]
["Ventilador","Presión estática externa","Nom.","Pa","40"]
["Power supply","Fase","","","1~"]
["","Frecuencia","","Hz","50/60"]
["","Nombre","","","VE"]
["","Tensión","","V","220-240"]
["Notas","","","","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar."]